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SAFE FUEL HANDLING
As a rule, all personnel handling fuel for their personal boats, club owned boats, and general use must follow the guidelines below:
	STANDARD OPERATING PROCEDURES - Fuel Handling

	Storage
	a) Gasoline must be stored in an approved container or tank in a well ventilated area like an outdoor shed. Do not store in glass or unapproved containers.

b) Keep it in a detached garage or shed and away from heat sources.

c) The club approved storage location is: [Insert storage location] 
d) Never leave a container of gasoline in direct sunlight or in the trunk of a car.

	When filling
	a) Do not smoke. 

b) Make sure engine is turned off.

c) In larger boats turn off auxiliary sources of ignition such as heaters, pilot lights and cooking units prior to refueling.

d) Portable containers must be placed on the ground and the nozzle must stay in contact with the container when filling to prevent buildup and discharge of static electricity.

e) Never siphon gasoline by mouth.

f) Fill containers no more than 95% full to allow for expansion.

g) Tighten both the fill cap and the vent cap on the container after filling.

	In Use
	a) Use gasoline as a motor fuel only.

b) Never use gasoline as solvent or cleaner.

c) Never use gasoline to start a fire or pour it on a fire that is already lit. The fire can rush back up the stream and ignite the container in your hand.

d) Never try to extinguish a gasoline fire with water. It will only spread the fire. Use a BC Class fire extinguisher.

e) Wait for lawnmowers, chain saws or any machinery to cool before refueling them.

f) Never use gasoline indoors.



	Caution
	Never pour gasoline on the ground, in a sewer or drain, or into a lake or river. Not only does it contaminate the environment, it may cause a fire or explosion. Unwanted gasoline must be taken to a hazardous waste disposal centre.


